VIN Decoding 1973 Wagoneer
The VIN is located on a plate mounted on the left corner of the firewall under the hood. 

Note: Beginning with the six digit serial number 100,000 the Alphabetical GVW rating code is replaced by the actual numerical weight designation. 

1st Digit - Manufacturer 

	J- Jeep Corporation


2nd Digit - Model Year 

	3- 1973


3rd Digit - Plant/Transmission/Drive Code 

	A- Toledo, Hydramatic-LHD

	B- CKD (Complete Knock Down), Hydramatic-LHD

	F- Toledo, 3-Speed-LHD

	G- Toledo, 3-Speed-RHD

	J- CKD, 3-Speed-LHD

	K- CKD, 3-Speed-RHD

	M- Toledo, 4-Speed-LHD

	N- Toledo, 4-Speed-RHD

	O- CKD, 4-Speed-LHD

	P- CKD, 4-Speed-RHD 


4th & 5th Digit - Series 

	14- Wagoneer-110" Wheelbase

	15- Wagoneer-Custom-110" Wheelbase

	25- Truck- 119" Wheelbase

	26- Truck- (Export Only), 119" Wheelbase

	45- Truck- 132" Wheelbase

	46- Truck- 132" Wheelbase

	47- Truck-132" Wheelbase

	48- Truck-132" Wheelbase


6th Digit - Body Style 

	1- Thriftside-Pickup

	2- Townside-Pickup

	4- 4 Door Wagon

	6- Cab and Chassis

	7- 2 Door Wagon

	8- Stripped Chassis


7th Digit - GVW/Model 

	C- 5600 

	E- 6000 

	K- 7200 

	M- 6500

	W- 5000

	X- 6000

	Y- 7000

	Z- 8000 


8th Digit - Engine 

	A- 6-258 Regular

	N- V8-360 2V

	P- V8-360 4V

	Z- V8-401 4V


9th thru 13th Digit - Sequential Serial Number 

	00001-99,999


References: 

	Parts Manual: W-1170-R2, Kaiser Jeep Corporation, 1967

	Parts Manual: F-76072, AMC, Feb 1972

	Parts Manual: F-75080, AMC, May 1980

	Parts Manual: 89-81-374-084, AMC, May 1987


